Gigabit Ethernet Switch, 4xLAN, incl. 6VDC plug-in power supply, bidirect to SC/APC

Gigabit Ethernet Switch, 4xLAN, incl. 6VDC plug-in power supply, bidirect to SC/APC,

FTTx customer terminal, Gigabit Ethernet switch for XON30. The module is available in different versions, each for 1- and 2-fiber topologies.

Optimal solution for housing industry, city network operators or energy and utility companies. By inserting the XON1300.S into the XON30 wall bracket, the end customer can commission the connection. Excellent quality and workmanship guarantee longevity and reliability in order to be prepared for future bandwidth requirements.

Supplied without empty housing.

Number of 10/100/1000 Mbps RJ45 ports: 4

Mounting type: Empty chassis

Ethernet: Yes

Fast Ethernet: Yes

Gigabit Ethernet: Yes

10 Gigabit Ethernet: No

Make: BKtel

Item no.: XON1300.S