INFRALAN® SC coupling in metal housing

INFRALAN® SC coupling in metal housing,

The INFRALAN® SC Duplex coupling in metal housing complies with DIN EN 61754-4. Due to the metal housing it has a higher stability and a low sensitivity to temperature fluctuations. Mounting options include clips or enclosed M2 threaded screws, incl. dust caps.

Connector type 1st side: LC Duplex

Connector type 2. side: LC Duplex

Material: metal

Type of mounting: screw/engagement

Sleeve material: Ceramic

Design: SC-Duplex

Operating temperature: -40 to 85°C

Storage temperature: -40 to 85°C

Dimensions: hxbxt 9,4x34,7x27,4mm

Make: INFRALAN®

Item no.: IKL-SCDU-M-SI