INFRALAN® Cat.6A Installation U/UTP 500 MHz, CPR B2ca

INFRALAN® Cat.6A Installation U/UTP 500 MHz, CPR B2ca,

Data installation cable with massive copper conductors (AWG23). For the use in structured buildings cabling according to EN 50173, ISO/IEC 11801. Data-cable for transmission up to 500MHz, for electrical transmission with the requirements for category 6A, transmission of 10GBit Ethernet are easily possible, two leads twisted as a couple, 8 leads designated with colour according to TIA/EIA 568-C2, harmonised norm EN 50575, halogen free according to EN 60754, low in smoke according to EN 61034, flame-retardant according to EN 60332-3-24 (FRNC-C), EURO-class B2ca-s1a, d0, a1.

Cable structure: U/UTP

Conductor category: Kl.1 = single wire

NVP-value: 68,2%

Operating temp. flexible: 0 bis 60°C

Operating temperature,fix: -15 bis 75°C

Outer diameter: 6,6mm

Tractive Force: 110N

Color outer sheath: RAL5015, blue

Length: 305m (box)

Brand: INFRALAN®

Item No.: 99965.305-CPR