INFRALAN® Consolidation Point Cable KOP

INFRALAN® Consolidation Point Cable KOP,

consists of three following components of the INFRALAN® program:

INFRALAN® RJ45 connection module Cat.6a/Class EA (IKS-6A-KOP-XX), INFRALAN® Cat.7A laying cable S/FTP 1200 MHz CPR Cca as simplex cable with 4x2xAWG23/1 (99985.x-CPR) and the INFRALAN® Cat.6A field-attachable RJ45 connector STP (IVB-6A-S), component certified by GHMT.

These are combined in one cable and thus offer a flexible variant for producing a 4 connector link.

Category: 6A

Application: 10 Gigabit Ethernet

Plug connector 1st side: RJ45 plug IVB-6A-S

Connector 2nd side: RJ45 Keystone IKS-6A-KOP-XX

Coat colour: yellow

Flame retardancy according to: EN60332-1

Length: 5,0m

Make: INFRALAN®

Item no.: ICP-6A-KOP-0500

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

INFRALAN® Consolidation Point Cable KOP

INFRALAN® Consolidation Point Cable KOP,

as described above, however:

Length: X,Xm

Make: INFRALAN®

Item no.: ICP-6A-KOP-XXXX

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Structure Art. no:

ICP-6A-KOP-XXXX

-XXXX = Length = "0500" = 5,0m

Available in lengths:

5,00m / 10,00m / 15,00m