FTTH indoor connection box for 2 fibres, 2 couplings

FTTH Indoor connection box for 2 fibres, 2 couplings,

unassembled 2-port connection box made of plastic suitable for SC-Simplex/ LC-Duplex/ E2000® couplings, which has an overlength fibre holder and a plug protection device. The FTTH indoor connection box is used in optical telecommunication networks, LAN, CATV networks, FTTH networks as well as PON and G-PON.

Supplied with 2x shrink splice protection and material for wall mounting. When using crimp splice protection, please note that it cannot be permanently inserted.

Application: Indoor

Mounting type: Wall mounting

Possibility of mast mounting: No

Material: plastic

Colour: White

Maximum number of fibres: 2

splice protection type: shrink / crimp

Coupling type: SC Simplex/LC Duplex/E2000®

Max. Equipment (adapter): 2

IP Protection class IP20

Protection against foreign bodies and accidental contact: Protection against medium-sized foreign bodies

Water protection: No protection

Dimensions: hxbxt 84mm x 130mm x 24mm

Temperature range: 0°C - 50°C

Access protection: Without

Make: EFB-Elektronik GmbH

Item no.: FTTH-BOX-IN-2