INFRALAN® wall-mounted enclosure 6HE, 3-part, RAL7035, 600mm

INFRALAN® wall-mounted enclosure 6HE, 3 parts, RAL7035, 600mm,

19" wall-mounted enclosure as three-part sheet steel enclosure with welded frame, completely pre-assembled, self-ventilated. Swivel frame on the rear side for folding out the front part of the housing. Roof and floor with pre-punched cut-outs for cable entry, prepared for installation of 2x individual ventilators each in roof and floor. Inside front side 2x 19" struts, galvanized and depth adjustable, L-shaped. One front door with viewing window made of certified safety glass and with sash fastener. Cabinet parts completely earthed on the inside.

Accessories included: 1x brush strip, 1x cage nut set (20 pcs.), 2x wrench

Height units: 6HE

Front door: glass, 1-piece

Protection class: IP20

Colour: RAL7035, light grey

Load capacity: 40kg

Dimensions: hxbxt 330x600x600mm

Make: INFRALAN®

Item No.: IWG-0666S.GR