Coupling LC Duplex SM Metal Housing, ceramic sleeve

Coupling LC Duplex SM metal housing, ceramic sleeve,

LC-Duplex couplings in metal housing, which fit into SC-Simplex cut-outs. The couplings can be fixed with clips or M2 threaded screws, which are included in the scope of delivery.

Connector type Connection 1: LC-Duplex

Connector type Connection 2: LC duplex

Design: SC-Simplex

Dust protection flap: Yes

Accessories: Metric screw

Housing material: Metal

Type of mounting: screw/engagement

Sleeve material: Ceramic

length: 29,2 mm

width: 22 mm

height: 9,5 mm

Operating temperature: -40°C - 85°C

Storage temperature: -40°C - 85°C

Conforms to standard: IEC 61754-20

Colour: Metal

Suitable for fiber type: Singlemode

Version: LC / PC

Insertion loss 1310nm: < 0.25 dB

Make: EFB-Elektronik GmbH

Item no.: 53343.1