INFRALAN® RJ45 keystone UTP Cat.6A / Class EA

INFRALAN® RJ45 keystone UTP Cat.6A / Class EA,

RJ45 module in white plastic housing (PC + ABS), Cat.6A component certified according to ANSI/TIA-586-C.2 and ISO/IEC 11801, simply toolless assembly, cable presorter for AWG24/1 - AWG22/1, pair management according to TIA/EIA 568 A/B, IEEE802.3af/at/bt, appropiated for frames and distribution panels with keystone slots, ANEXT optimized with INFRALAN®-distribution panel IVF-24-SW-UTP, including cabel tie, mounting instruction and hinged dust cover.

Mating cycles: > 750

Cabel diameter: max. 8,5mm

Contact coating: 50μ“ gold plated

Contact resistance: < 20 mΩ

Current rating: 2A @ 20°C

Temperature range: -40°C bis +66°C

Brand: INFRALAN®

Item No.: IKU-6A-KOP-1