INFRALAN® cable connector Cat.6A / Class EA 10Gbit/s

INFRALAN® cable connector Cat.6A / Class EA 10Gbit/s,

Cable connector for Link Performance 10 Gbit/s Class EA according to ISO 11801Ed.2.2 (2011-06) for connecting installation cables e.g. in parapet ducts or cable ducts as well as in connection with patch cables for end-to-end links or in consolidation point applications, fully shielded housing made of die-cast zinc, small space requirement due to compact design (dim.: hxbxt 26x18x39mm), simple assembly without special tools, universal mounting options by screwing and stringing together via an optionally available 19" carrier panel for up to 24 connectors. PoE according to IEEE802.3af/at/ bt, independent 360° shield contacting and strain relief of the cable by means of sliding mounted shield contacting for different cable diameters.

Scope of delivery: 1x connector, 2x cable pre-sorter for AWG26/1 to AWG22/1 as well as AWG26/7 to AWG24/7 with pair management via colour code (printed on the cable pre-sorter), 2x copper foil, 2x cable ties.

Make: INFRALAN®

Item no.: IVB-6A-V