INFRALAN® 1-Port RJ45 Keystone Holder for DIN Rail Mounting

INFRALAN® 1-Port RJ45 Keystone holder for DIN rail mounting,

Plastic module support is suitable for mounting on top-hat rail TH35 according to DIN EN 60715 and has a width of 1 TE. The end plate included in the scope of delivery serves to protect against contact and to complete the series. The module holder can accommodate an INFRALAN®-Keystone module and can be mounted in an unlimited number of rows.

Mounting type: DIN rail 35 mm

Type: diagonal (mounting rail adapter)

Material: plastic

Colour: RAL7035, grey

Make: INFRALAN®

Item no.: IMT-01-HS-GR