ISDN Patch Panel 19" 1U 50port, unshielded, Cat.3

ISDN Patch Panel 19" 1U 50port, unshielded, Cat.3,

4-pin LSA Terminals, RJ45 8(4) jacks, high packing density, strain relief via cable ties, for AWG 22 – 26 cable, RJ45 jack housing PBT/ UTP, UL94-V0

Assignment: 3-6/4-5

IDC Body: Fireproof PC/ ABS UL-94V0

IDC Contakt: Bronze and tinned

Isolation resistance: ≥ 500 MΩ

Contakt resistance: ≤ 20mΩ

Current rating: 1,5A

Withstanding voltage:1000 VAC RMS 60Hz/1 min.

Color: grey, RAL 7035

Make: EFB-Elektronik

Art.-No.: 37595.2