INFRALAN® U-DQ(ZN)BH 4E 9/125µ G652.D

INFRALAN® U-DQ(ZN)BH 4E 9/125µ G652.D,

Universal Cable, Singlemode G652.D, for fix application indoor and outdoor in plastic pipe systems, cable ducts and on platforms.

Material outer sheath LSZH coloured in black, metal free, longitudinal water blocking, Halogen free,
central loose tube filled with gel, multifunctional Glasroving wrapping, two-layered,
as stain relief element and non-metal rodent protection.

Harmonised Norm: EN 50575, halogen free according to EN 60754-1/2, low in smoke according to EN 61034-2, flame-retardant according to EN 60332-1, EURO-fire protection class Dca-s2, d2, a2.

Outer diameter: 6,0mm

Tensile, long term: max. 1500N

Crush resistance: 150N/cm

Bending radius: 60mm

Operating temperature, moved: -5 to 50°C

Operating temperature, dormant: -20 to 60°C

IL, max. 1310nm: 0,36db/km

IL, max. 1550nm: 0,22db/km

Rayleigh Backscatter Coefficient 1310nm: 1,4676

Rayleigh Backscatter Coefficient 150nm: 1,4682

Construct: 04E (1x4) Singlemode G652D

VDE-Name: U-DQ(ZN)BH 4E9/125

Fabricate: INFRALAN®

Art.-No.: 54404.1A-CPR