INFRALAN® Wall enclosure 4HE, 3 parts, RAL7035, 500mm

INFRALAN® wall enclosure 4HE, 3 parts, RAL7035, 500mm,

19" wall-mounted enclosure as three-part sheet steel enclosure with welded frame, completely pre-assembled, self-ventilated. Swivel frame on the rear side for folding out the front part of the housing. Roof and floor with pre-punched cut-outs for cable entry, prepared for installation of 2x individual ventilators each in roof and floor. Inside front side 2x 19" struts, galvanized and depth adjustable, L-shaped. One front door with viewing window made of certified safety glass and with sash fastener. Cabinet parts completely earthed on the inside.

Accessories included: 1x brush strip, 1x cage nut set (20 pcs.), 2x wrench

Height units: 4HE

Front door: glass, 1-piece

Protection class: IP20

Colour: RAL7035, light grey

Load capacity: 30kg

Dimensions: hxbxt 240x600x500mm

Make: INFRALAN®

Item no.: IWG-0465S.GR