FTTH Indoor Box for 4 adapters, crimpversion

FTTH Indoor Box for 4 adapters, crimpversion   
unassembled 4-port connection box made of plastic suitable for SC-Simplex/ LC-Duplex couplings, equipped with cable guide. The FTTH indoor connection box is used in optical telecommunication networks, LAN, CATV networks, FTTH networks as well as PON and G-PON.  
Suitable for drop-cables to splice inside the box with pigtail and capable for the installation of different lengths of pre terminated drop-cables with LC and SC connectors.

Scope of application: inside  
Mounting: wall mounting-/DIN Rail  
Mast installation: false  
Material: plastic  
Colour: white  
Maximum assembly: 4 adapters  
Splice protection: crimp  
Suitable for adapters: SC Simplex/LC Duplex  
IP protection IP20  
Forgein body and contact protection: Protection against medium sized forgein bodies  
Water protection: No portection  
Dimensions: 80mm x 80mm x 28mm

Manufacturer: EFB-Elektronik GmbH  
Item-No.: FTTH-BOX-IN-6