INFRALAN® FO frame set, 2-fold, RAL 9010

INFRALAN® FO frame set, 2-fold, RAL 9010,

for flush-mounted or duct connection, base element with central cover plate for accommodating 2 fibre optic feed-through couplings (SC simplex, LC duplex, E2000® simplex), 40° outlet, central plate to DIN49075, compatible with various standard switch ranges via intermediate frame, mounting frame with plastic cover 80x80mm, central plate 50x50mm, colour RAL 9010 pure white, with dust protection cap, labelling field and connection option for equipotential bonding.

Make: INFRALAN®

Item no.: IMT-02-RL-WS-KP