INFRALAN® Patchbox for Keystones

INFRALAN® Patchbox for Keystones,

the INFRALAN® Patchbox in 19"/1HE with its closed metal housing in grey and extendable front, offers the possibility to accommodate up to 24 modules in Keystone format due to its modular design. The INFRALAN® Keystone IKS-6A-PVP can be fully equipped. The connection option for earthing cables, strain relief via cable ties and the sequential port numbering 1 - 24 round off the wide range of possible applications of this patchbox. The patchbox has the dimensions hxbxt 445x483x244mm and cable glands at the rear.

Make: INFRALAN®

Item no.: ISB-KS-24-GR