Industrial splice distributor for DIN-RAIL

Industrial splice distributor for DIN-RAIL, metal housing without front panel. Cable entries on top and buttom each prepared for M20 cable gland, delivery includes splice holder for 12 crimp splices and splice cassette.

Combinable with EFB front plates 53705.3V2B (6 x LC duplex, SC simplex, E2000®),   
53705.2V2B (6 x SC duplex /LC quad), 53705.3V4B (12 x LC duplex, SC simplex, E2000®),   
53705.5V2B (12 x ST simplex).

color: RAL 7035

dimension: 61x115x113mm

manufacturer: EFB-Elektronik

Item-No.: 53705.1V3